**# Terminal**

[ReqId:01v01]: It shall be possible to have a <terminal> application in order to interact with the user over USB.

[ReqId:02v01]: <terminal> shall have a menu system as the user interface.

[ReqId:03v01]: The user of <terminal> shall be able to set <time> and <date> of the RTC.

[ReqId:04v01]: The user of <terminal> shall be able to get <time> and <date>.

**# Display**

[ReqId:05v01]: It shall be possible to have a <Display> application in order to interact with the user over SPI.

[ReqId:06v01]: <Display> shall be able to display current <time> in two different format, that is digital and analog

[ReqId:07v01]: <Display> shall be able to display current <date>.

Application Layer: 01, 02, 03, 04, 05, 06, 07

Abstraction Layer: 01, 03, 04, 05, 06, 07

IoHwAb:

COM stack: 01, 03, 04, 05, 06

Memory Service:

RTOS: 06, 07